CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2.3/conf/instr/AVII400/uxnmr.info
Date         : Fri Nov 08 10:58:44 2013
Release      : TOPSPIN Version 3.2-pl3
Installed in : C:/Bruker/TopSpin3.2.3
Host         : CZC3047DYB
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 3591 MHz with Hyperthreading)
User         : nmr
Description  : Avance-AV 400
Location     : University of Southampton
System       : Avance-AV NMR spectrometer
1H-frequency : 400.13 MHz
Order Number : GH004413
Configured in: C:/Bruker/TopSpin3.2.3/conf/instr/AVII400

#--------------------
#  FCU configuration:
#--------------------
board # 1 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 2 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)

DRU: AQS DRU Z100977/00636 ECL 04.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419

Gcu: GCU3_SlowIF

AQS: connected to AVII400:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x62   0x1    AW  R  0.0 REC-1  AQS RXAD-400 Z102116/00012 ECL 0.0
     4   0x24 0x10   0x4    BH  S  6.3 SGU-1  AQS SGU400 Z003642/04482 ECL 6.3
     5   0x25 0x10   0x4    BH  S  5.0 SGU-2  AQS SGU400 Z003642/03317 ECL 5.0
     9   0x36  0x5     0        A  5.0 BLA-1  BLA2BB 150/60 20-400 W1345049/1401 ECL 5
    11   0x1a  0x9     0        C  3.0 ACB-S  ACB Standard
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 AQS-Minirouter


Amplifiers (AQS configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        B      150    N         BLA2BB 150/60 20-400 W1345049/1401/-
   2      1         2        B       60    N         BLA2BB 150/60 20-400 W1345049/1401/-
   3      2         1       2H       20    N         BSMS 2HTX -/-/-



- Type: BSMS/1
- absolute lockshift frequency = changed from 11433137 Hz to 11422391 Hz Hz
- 2HTX Amplifier: connected to router output 3
- GAB type = GAB
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)

Bruker Automatic Changer: device connected to AVII400:/dev/tty08
- Capacity: 60 holders
- Firmware: 19990701
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Lock: device connected to AVII400:/dev/tty03

Eurotherm VTU: device connected to AVII400:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to AVII400:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AP
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H/2H 1H (virtual 50 Ohm reference: 269.9%/86.9deg)
                 PN=Z003959, SN=00128 from 20090406
    Module  2 : 1H/2H 2H (virtual 50 Ohm reference: 104.0%/-67.9deg)
                 PN=Z003959, SN=00128 from 20090406
    Module  3 : XBB19F 2HS
                 PN=Z003504, SN=00111 from 20041109


Frequency generation:
- F1: for SGU
- F2: for SGU



