files o2-40-ar-28-3s-spectra show the measured spectrum that was used for ptychography reconstruction

ptycho_data.mat contains the ptychography data and basic parameters of the ptychography scan. Data are unprocessed raw diffractions and position of the collected regions are in nm. 

