# Descriptions for all the data shown in this folder

Two models are shown in this folder to demonstrate the modelling of boundary-driven streaming patterns in acoustofluidic devices using the Reynolds stress method and the limiting velocity method, respectively.

The numerical method and procedures have been explicitly described in the paper, titled “comparing methods for the modelling of boundary-driven streaming in acoustofluidic devices”.