CONFIGURATION INFORMATION
=========================

Path         : /opt/PV6.0.1/conf/instr/spect/uxnmr.info
Date         : Wed Dec  5 11:53:48 2018
Release      : TopSpin Acquisition Version 3.1PV beta-pl1
Installed in : /opt/PV6.0.1
Host         : floke
OS           : CentOS Linux release 7.5.1804 (Core) 
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 3775 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
Description  : AVIII 500WB
Location     : University of Southampton
System       : Avance III NMR spectrometer
1H-frequency : 500.10 MHz
Order Number : GH003212
Configured in: /opt/PV6.0.1/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 6
- Gctrl1: with digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU: AQS DRU-E Z102520/04020 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  5.0 REC-1  AQS RXAD600 Z102117/1141 ECL 05.00
     3   0x34 0xc9   0x1        X  1.3 REF-1  REF/2-1000 Reference Board for AQS/2 Receiver
     4   0x24 0x19   0x8    AE  S  2.7 SGU-1  AQS SGU/2 600 Z103081/02549 ECL 02.07 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.4 SGU-2  AQS SGU/2 600 Z103081/01093 ECL 02.04 FPGA-Vs=AF
     6   0x26 0x19   0x8    AE  S  2.1 SGU-3  AQS SGU/2 600 Z103081/00753 ECL 02.01 FPGA-Vs=AF
     7   0x27 0x19   0x8    AE  S  2.7 SGU-4  AQS SGU/2 600 Z103081/02550 ECL 02.07 FPGA-Vs=AF
     8   0x28 0x19   0x8    AE  S  2.7 SGU-5  AQS SGU/2 600 Z103081/02551 ECL 02.07 FPGA-Vs=AF
     9   0x29 0x19   0x8    AE  S  2.3 SGU-6  AQS SGU/2 600 Z103081/00986 ECL 02.03 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0237 W1345093/0237 ECL 1:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0237 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0791 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/0459 ECL 03
BLA_W1345093_0657 W1345093/0657 ECL 12:
- TCP/IP address = 149.236.99.92
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0657 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2452 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7576 ECL 50
BLA_W1345087_0057 W1345087/0057 ECL 1:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAH300 E 200-600MHZ INR: W1345087/0057 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0792 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00600 ECL 03

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGAU_W1522066_0178
- TCP/IP address   = 149.236.99.94
- Firmware version = 20141128
- Web version      = 2.1
- Current limits   = 60.0/X, 60.0/Y, 60.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20170712
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS-WB
- 2HTX Amplifier: available
- Lock: installed
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00237 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01653 ECL 01.04

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.9%/0.5deg, reflection meter)
                 PN=Z103204, SN=00081 from 20110407
    Module  2 : 1H LNA
                 PN=Z003461, SN=00998 from 20110323
    Module  3 : 2H
                 PN=Z003472, SN=00944 from 20110328
    Module  4 : XBB19F 2HS
                 PN=Z003505, SN=01025 from 20110401
    Module  5 : XBB19F 2HS
                 PN=Z003505, SN=108 from 20010912


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU
- F5: for SGU
- F6: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0237 at TCP/IP 149.236.99.93)
SGU1 AUX  output -> input 1 of transmitter 4 (BSMS 2HTX)
SGU2 NORM output -> input 1 of transmitter 3 (BLAH300 E 200-600MHZ INR W1345087/0057 at TCP/IP 149.236.99.91)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0657 at TCP/IP 149.236.99.92)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0237 at TCP/IP 149.236.99.93)
SGU4 NORM output -> input 2 of transmitter 3 (BLAH300 E 200-600MHZ INR W1345087/0057 at TCP/IP 149.236.99.91)
SGU4 AUX  output -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0657 at TCP/IP 149.236.99.92)
SGU5 NORM output -> open
SGU5 AUX  output -> open
SGU6 NORM output -> input 3 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0657 at TCP/IP 149.236.99.92)
SGU6 AUX  output -> open

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0237 at TCP/IP 149.236.99.93) amplifier X-500W uses blanking 1
transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0657 at TCP/IP 149.236.99.92) amplifier X-500W uses blanking 3
transmitter 3 (BLAH300 E 200-600MHZ INR W1345087/0057 at TCP/IP 149.236.99.91) amplifier 1H-300W uses blanking 2
transmitter 3 (BLAH300 E 200-600MHZ INR W1345087/0057 at TCP/IP 149.236.99.91) amplifier 1H-50W uses blanking 2
transmitter 4 (BSMS 2HTX) amplifier 2H-20W needs no blanking

Preamplifier connections (detected by 'confrecpre')
--------------------------------------------------------------------
Tune-SGU2 -> HPLNA 19F1H -> REC1
Tune-SGU2 -> 1H LNA      -> REC1
Tune-SGU2 -> 2H          -> REC1
Tune-SGU2 -> XBB19F 2HS  -> REC1
Tune-SGU2 -> XBB19F 2HS  -> REC1

