Folder contains raw data files for panels (b,c,e,g,h) in Fig. S8 in the supplementary information. 

Each datafile contains three number-columns corresponding to each datacurve in Fig. S8. First column refers to the time (horizontal axis) coordinate (in nanoseconds); second column is the area integrated Stokes component (vertical axis coordinate); the third column is the area integrated S1 Stokes component corresponding to the marker color.

Datafiles that are labeled with "H" refer to horizontally polarized initial condition. Datafiles that are labeld with "V" refer to vertically polarized initial condition.

 