Folder contains raw data files for each panel in Fig. 2. 


Files contain seven columns and the Stokes parameters (S1, S2, S3) should be plotted versus the first column values (Pump Power (P/Pth). Columns dS1, dS2, dS3 are the error values and should be plotted as the error bars for the corresponding Stokes parameters. 