Folder contains raw data files for each panel in Fig.3. 


File fig3a.txt contains seven columns and the Stokes parameters ( titled S1, S2, S3) should be plotted versus the first column values (PL major axis angle (deg.)). Columns dS1, dS2, dS3 are the error values and should be plotted as the error bars for the corresponding Stokes parameters. 
Files fig3b.txt and fig3c.txt contains three columns and should be plotted as an "intensity map", with x- and y- values of each pixel on the map corresponding to the values of the first (PumpPower(p/pth)) and the second (Pl Major axis angle (deg.)) columns respecyievly, the values of the third values are the S1 and S2 values for the corresponing polarization map.