Folder contains raw data files for each panel in Fig. S3 in the supplementary information. 


File figS3a.txt contains four columns and the Stokes parameters ( titled S1, S2, S3) should be plotted versus the first column values (PL major axis angle (deg.)). 
Files fig3b--e.txt contain three columns and should be plotted as an heatmap, with x- and y- values of each pixel on the map corresponding to the values of the first (PumpPower(p/pth)) and the second (Pl Major axis angle (deg.)) columns respecyievly, the values of the third values are the S1, S2 and S3 values for the corresponing polarization map.