Dataset for L. K. Piper et al., Mechanically Tunable Terahertz Metamaterial Perfect Absorber
Advanced Photonics Research 2021, DOI: 10.1002/adpr.202100136

Dataset consists of raw data for figures with following formats
Figure 1: no associated data

Figure 2:
figure2a_exp1reflectivity.txt : columns of ascii data with frequency (1st column), reflectivity in dB for different cavity thickness (2+ column)
figure2b_exp2reflectivity.txt : columns of ascii data with frequency (1st column), reflectivity in dB for different cavity thickness (2+ column)
figure2c_simreflectivity.xlsx : excel sheet with columns of ascii data with different sets of frequency (columns A, D, K, M, O) and reflectivity in dB for different cavity thickness
figure2d_exp1.dat : comma-separated ascii data with cavity thickness in micrometer (1st column), resonance frequency (GHz), normalized f/f0
figure2d_exp2.dat : comma-separated ascii data with cavity thickness in micrometer (1st column), resonance frequency (GHz), normalized f/f0
figure2d_sim.dat : comma-separated ascii data with cavity thickness in micrometer (1st column), resonance frequency (THz), normalized f/f0
figure2ef_exp1.dat : comma-separated ascii data with cavity thickness in micrometer (1st column), reflectivity at minimum (dB), reflectivity at minimum (linear)
figure2ef_exp2.dat : comma-separated ascii data with cavity thickness in micrometer (1st column), reflectivity at minimum (dB), reflectivity at minimum (linear)
figure2ef_sim.dat : comma-separated ascii data with cavity thickness in micrometer (1st column), reflectivity at minimum (dB), reflectivity at minimum (linear)

Figure 3:
figure3a_exp1refldB.txt : ascii data for 2D maps with cavity thickness in micrometer (1st row), frequency (GHz) first column, 2D matrix of reflectivities (dB)
figure3b_exp2refldB.txt : ascii data for 2D maps with cavity thickness in micrometer (1st row), frequency (GHz) first column, 2D matrix of reflectivities (dB)
figure3c_range1.xlsx : excel sheet with data for 2D maps with cavity thickness in micrometer (1st row), frequency (GHz) first column, 2D matrix of reflectivities (linear)
figure3c_range2.xlsx : excel sheet with data for 2D maps with cavity thickness in micrometer (1st row), frequency (GHz) first column, 2D matrix of reflectivities (linear)
figure3c_range3.xlsx : excel sheet with data for 2D maps with cavity thickness in micrometer (1st row), frequency (GHz) first column, 2D matrix of reflectivities (linear)

Figure 4:
figure4a_exp1phase.txt : columns of ascii data with frequency (1st column), phase for different cavity thickness (2+ column)
figure4b_exp2phase.txt : columns of ascii data with frequency (1st column), phase for different cavity thickness (2+ column)
figure4c_simphase.txt : columns of ascii data with frequency (1st column), phase for different cavity thickness (2+ column)

Figure 5:
figure5a_exp1phase.txt : ascii data for 2D maps with cavity thickness in micrometer (1st row), frequency (GHz) first column, 2D matrix of phases
figure5b_exp2phase.txt : ascii data for 2D maps with cavity thickness in micrometer (1st row), frequency (GHz) first column, 2D matrix of phases
figure5c_simphase.txt : ascii data for 2D maps with cavity thickness in micrometer (1st row), frequency (GHz) first column, 2D matrix of phases
