READ ME File For 'DATASET for a TEAS measurement of hexane (the solvent). The sample was pumped at 200 nm and probed between 350 nm to 700 nm'

Dataset DOI: https://doi.org/10.5258/SOTON/D2658

Date that the file was created: 14/06/23 (DD/MM/YY)

-------------------
GENERAL INFORMATION
-------------------

ReadMe Author: Edward Plackett, University of Southampton

Date of data collection: 28/05/21 (DD/MM/YY)

Others credited for data acquisition: Russell Minns, Rebecca Ingle, Gabiriel Karras, Igor Sazanovic, Henrgy McGee

Information about geographic location of data collection: ULTRA, CLF, Rutherford Appleton laboratories, Didcot
--------------------------
SHARING/ACCESS INFORMATION
-------------------------- 

Licenses/restrictions placed on the data, or limitations of reuse: 6 month embargo then CC-BY

Publisher: University of Southampton, U.K

Abbreviations: TEAS is Transient Electronic Absorption Spectroscopy

--------------------
DATA & FILE OVERVIEW
--------------------

This zipped dataset contains the data used the analysis shown in section 4.3.3, showing the results of a time-resolved infrared measurement through a 200 nm pumped hexane solution, probed between 350 nm to 700 nm'

hexane_TEAS_info.txt contains information about the experimental conditions (sample, solvent, how many acquisition cycles were run)

hexane_TEAS_cycle1.csv contains the pixel x intensity data at the pump-probe delays specified in the top row of the file. hexane_TEAS_AvDiff.csv then contains the average of the cycle 1 measurements. 

Due to issues with the clibration taken on the day, a rough calibration was taken after our ULTRA experimental time - the calibration formula used is: 877-(pixel_number+34)*1.3358


