-------------------------------------------------------------------------------------------------------------------------------------------------------------
README - Research Data Set
Data Set Title: "Data and Code Repository for "An Image-Based Inertial Impact (IBII) Test for Tungsten Carbide Cermets""
DOI: 10.5258/SOTON/D0607
-------------------------------------------------------------------------------------------------------------------------------------------------------------
Associated Publication:
L. Fletcher and F.Pierron, An Image-Based Inertial Impact Test for Tungsten Carbide Cermets, Journal of Dynamic Behavior of Materials, 2018

-------------------------------------------------------------------------------------------------------------------------------------------------------------
Research Group: PhotoDyn Research Group (http://photodyn.org/)
Department / Institution: Mechanical Engineering, University of Southampton, UK
Principal Investigator: 
Prof. Fabrice Pierron
+44 (0)2380 592891
f.pierron@soton.ac.uk

Data Collector / Corresponding Author: 
Dr. Lloyd Fletcher
+44 (0)23 8059 6626
l.c.fletcher@soton.ac.uk

-------------------------------------------------------------------------------------------------------------------------------------------------------------
Data Collection Date: November 2017
License: Creative Commons-Non Commercial – Share Alike

Description: Matlab processing code, raw experimental images and processed data for Image-Based Inertial Impact (IBII) tests on tungsten carbide samples of various compositions. Processing code is enclosed in a single zip file. Data for experimental specimens are grouped by material grade identifier with all specimens from a single group being contained within a single zip file including raw images and processed data. Synthetic image deformation data is included in a separate zip file.

Data Files:
The following zip files contain the raw .tiff images for each sample based on the specimen identifier as described in the article listed at the top of this file. Each file also contains the processed data for each sample including: image sequences of the kinematic fields and identified material properties. 
•	Data_WC-C-13Co_S1.zip
•	Data_WC-C-13Co_S2.zip
•	Data_WC-C-13Co_S3.zip
•	Data_WC-F-6Co_S1.zip
•	Data_WC-F-6Co_S2.zip
•	Data_WC-F-6Ni_S1.zip
•	Data_WC-F-6Ni_S2.zip
•	Data_WC-F-6Ni_S3.zip
•	Data_WC-F-13Co_S1.zip
•	Data_WC-F-13Co_S2.zip
•	Data_WC-F-13Co_S3.zip

This file contains the Matlab code used to process the data and most of the dependent functions. The code uses the grid method toolbox which can be found here: http://www.thegridmethod.net/code
•	IBII_MatlabProcessingCode_v2_3.zip

This file contains the deformed grid images and an example processed output for the image deformation simulations.
•	SyntheticImageDeformationData.zip