READ ME File For 'DATASET for Broadband bismuth-doped fiber amplifier with a record 115-nm bandwidth in the O and E bands'

Dataset DOI:https://doi.org/10.5258/SOTON/D1119 

ReadMe Author: Yu Wang, Naresh K Thipparapu, David J Richardson, Jayanta Sahu, University of Southampton

This dataset supports the publication:
Yu Wang, Naresh K Thipparapu, David J Richardson, Jayanta Sahu. (2020)
Broadband bismuth-doped fiber amplifier with a record 115-nm bandwidth in the O and E bands
OFC 2020



Description:
The excel file contains all experimental data used for generating Fig.2 to Fig.3

The figures are as follows:

Fig. 2 (a)  Gain and NF spectrum from 1345nm-1460nm for a fixed signal power of -23dBm (the inset shows the signal and noise spectrum from which the in-band OSNR is derived); 

Fig. 2 (b)  Gain and NF variation with pump power for a -23dBm signal at 1420nm (where the slope of the dashed line represents the gain coefficient); 

Fig. 2 (c)  Gain and NF variation with signal power at 1420nm.

Fig. 3 (a)  Temperature dependent gain and NF characteristics from 1350nm-1460nm in the temperature range from -40 to +60 degreeC for a signal power of -23dBm; 

Fig. 3 (b)  Gain and NF from -40 to +60 degreeC at 1420nm for -23dBm signal (where the slope of dashed line represents the TDG coefficient).

Date of data collection 2019-11-20 to 2020-02-20

Related projects:
UK Engineering and Physical Sciences Research Council (EPSRC) under the “Airguide Photonics” Programme Grant (EP/P030181/1) 


Dataset available under a CC BY 4.0 licence


Publisher: University of Southampton, U.K.


Date: Feb 2020
