% See thesis for full description
% g = mass (g)
% cd20,cd10 = predicted uncertainty (at k=1) with l_r=50mm (ppm) for cd20, cd10 flexure bearings
% 20d40 = difference in predicted uncertainty (at k=1) between l_r=50mm and l_r=40mm (ppm) for cd20 flexure bearings
% 20d30 = difference in predicted uncertainty (at k=1) between l_r=50mm and l_r=30mm (ppm) for cd20 flexure bearings
% 10d40 = difference in predicted uncertainty (at k=1) between l_r=50mm and l_r=40mm (ppm) for cd10 flexure bearings
% 10d30 = difference in predicted uncertainty (at k=1) between l_r=50mm and l_r=30mm (ppm) for cd10 flexure bearings
g   cd20    cd10	20d40   20d30   10d40   10d30
10  207     207		-1      -3      0       0
5   306     304		-1      -7      0       0
2   376     371		-8      -35     0       0
1   561     547		-21     -89     0       -1